

 **RFP NO: FB21-041 DATE: MARCH 10, 2021**

 **BUYER: Kelly Sloan, Purchasing Manager PHONE: (816) 271-4465**

**ADDENDUM #1**

FUNDING DEPARTMENT: SCANLON HALL

EQUIPMENT/SERVICES REQUESTED: SCANLON HALL CARPET

**PLEASE NOTE: SEE BELOW FOR CLARIFICATIONS AND ADDITIONAL INFORMATION: PLEASE SUBMIT THIS INITIALED ADDENDUM WITH YOUR BID RESPONSE.**

1. What installation procedure should we follow to ensure the newly installed carpet remains under warranty? Please calculate this cost into your submitted bid price.

**PLATEX OR OLD ADHESIVES - Must be mechanically scraped down to a bare residue flat with the concrete substrate or covered with a skim coat of Portland cement-based patch reinforced with polymers. All old adhesive residue must also be covered with** [**Commercialon Premium Sealer**](file:///%5C%5CUNIV%5CNet%5CCommon%5CDepartments%5CPURCHASE%5CAddendums%5C2021%5CFB21-041%20Addendum%201%20Sealer%20Data%20Sheet.pdf)**. Note: Failure to remove or seal dissimilar adhesives may cause installation failure, plasticizer migration, shifting, buckling or edge curling; these conditions will not be covered under warranty.**

THIS ADDENDUM IS HEREBY CONSIDERED TO BE A PART OF THE ORIGINAL BID SPECIFICATIONS AND NEEDS TO BE INITIALED AND RETURNED WITH YOUR BID IN ORDER TO BE CONSIDERED.